Preventive Maintenance

**Daily**

Water tank level/swap

Sheets/Lines/Sails

Anchor rode/dock lines

Batt voltage

Clean Deck

**Weekly**

Generator checks

Engine checks

Changes in bilge levels

Cycle toilet salt system

Holding tank additive

Dinghy pressure

Wash Portlights/windows/hatches

Wash heads/shower strainers

Berth blinds/buttons

Water maker leaks

**Monthly**

Test All Light Sources

Test bilge pump

Clean/oil shroud swages

Verify pressure in accumulator tank

Check for fuel leaks around tanks

Check for mast base seepage

Inspect zincs

Inspect bottom paint

Check fire extinguishers

Inspect standing rigging

Inspect running rigging

Cycle all through hulls

Clean/polish stainless

Hose Clamps (double clamp thru-hulls)

Salon leather clean/treat

Inspect Propane Plumbing

Inspect Sails for Chafe

Inspect Batten Pockets

Clean/lubricate toilets

Check/defrost fridge/freezer

**Quarterly**

Inspect lifelines

Inspect batt Terminals

Tighten/replace all hardtop screws

Inspect Cleats

Drains and scuppers are clear

Clean Sun Shades and Cockpit Enclosure

Check mooring cleats/ground tackles, lines & fenders

Inspect hull/topside for nicks/cracks

Inspect swim ladder

Check shore power cables

Check PFDs

Check and clean shower sump filter screens

Clean/freshen fridge and cooler

Clean stove/verify all burners function

**Annually**

Service winches

Inspect/survey rigging

Inspect stanchions/pulpits/lifelines

Service sea strainers

Service water maker

Service engine

Service outboard motor

Check spare parts

Check tools

Verify Registration/Radio License/Insurance Dates

Replace Zincs

Check Rudders and Fittings/bearings

Repair hull/topside Nicks/Cracks

Check/repaint hull paint

Clean/service anchor windlass

Check davit cables for wear

Service/replace davit winch

Lubricate/service thru-hulls

Load test/replace batteries

Check galvanic isolator system

Inspect wiring for wear and chafe

Test all gauges and instrument

Inspect antennas

Check distress signal expiry

Check radar reflector

Check/replace first aid supplies

Check Liferaft date for service

Flush and clean water tanks

Inspect Steer for wear/chafe and lubricate

Inspect all lines/sheet/halyards for wear/chafe

Inspect fenders for wear/inflate